# :MEASure:VERTical:VTIMe:UREFerence:VALue

Amplitude-at-Time Commands

- :MEASure:VERTical:VTIMe
- :MEASure:VERTical:VTIMe:FAVorite
- :MEASure:VERTical:VTIMe:LOCation?
- :MEASure:VERTical:VTIMe:REGion
- :MEASure:VERTical:VTIMe:SOURce
- :MEASure:VERTical:VTIMe:STATus?
- :MEASure:VERTical:VTIMe:STATus:DETails?
- :MEASure:VERTical:VTIMe:STATus:REASon?
- :MEASure:VERTical:VTIMe:TIME
- :MEASure:VERTical:VTIMe:UREFerence:STATe
- :MEASure:VERTical:VTIMe:UREFerence:VALue

## Command Syntax

    :MEASure:VERTical:VTIMe:UREFerence:VALue <time_location>

<time_location> is a double.

## Query Syntax

    :MEASure:VERTical:VTIMe:UREFerence:VALue?

## Description

When a user-defined horizontal reference location is enabled (see `:MEASure:VERTical:VTIMe:UREFerence:STATe`), this command specifies its time location with respect to the trigger (t = 0) location.