# :MEASure:PAM:RFTime

PAM Rise/Fall Times Commands

- :MEASure:PAM:RFTime
- :MEASure:PAM:RFTime:EDIRection
- :MEASure:PAM:RFTime:FAVorite
- :MEASure:PAM:RFTime:LOCation?
- :MEASure:PAM:RFTime:OCCurrences
- :MEASure:PAM:RFTime:REGion
- :MEASure:PAM:RFTime:SOURce
- :MEASure:PAM:RFTime:STATus?
- :MEASure:PAM:RFTime:STATus:DETails?
- :MEASure:PAM:RFTime:STATus:REASon?
- :MEASure:PAM:RFTime:TRANsition
- :MEASure:PAM:RFTime:UREFerence:STATe
- :MEASure:PAM:RFTime:UREFerence:VALue

## Command Syntax

    :MEASure:PAM:RFTime

## Query Syntax

    :MEASure:PAM:RFTime?

## Description

Measures the rise time or fall time for the specified PAM signal level-to-level transition (see `:MEASure:PAM:RFTime:TRANsition`). For example in PAM4, there are six possible level-to-level transitions (`TRANsition01`, `TRANsition02`, `TRANsition03`, `TRANsition12`, `TRANsition13`, and `TRANsition23`).

Whether a rising edge or a falling edge is measured is specified by the `:MEASure:PAM:RFTime:EDIRection` command.