# :CMODe:THReshold:GENeral:LOWer

:CMODe Threshold Commands

- :CMODe:TBASe:GENeral:METHod
- :CMODe:TBASe:RFALl:METHod
- :CMODe:THReshold:GENeral:AUTO
- :CMODe:THReshold:GENeral:BASE
- :CMODe:THReshold:GENeral:COPY
- :CMODe:THReshold:GENeral:HYSTeresis
- :CMODe:THReshold:GENeral:LOWer
- :CMODe:THReshold:GENeral:METHod
- :CMODe:THReshold:GENeral:MIDDle
- :CMODe:THReshold:GENeral:PAM:ASLevels
- :CMODe:THReshold:GENeral:PAM:ASTHresholds
- :CMODe:THReshold:GENeral:PAM:PAMLevel:LEVel
- :CMODe:THReshold:GENeral:PAM:THResholds:EYE
- :CMODe:THReshold:GENeral:PLOWer
- :CMODe:THReshold:GENeral:PMIDdle
- :CMODe:THReshold:GENeral:PUPPer
- :CMODe:THReshold:GENeral:STZero
- :CMODe:THReshold:GENeral:TOP
- :CMODe:THReshold:GENeral:TRACking
- :CMODe:THReshold:GENeral:UPPer
- :CMODe:THReshold:RFALl:BASE
- :CMODe:THReshold:RFALl:COPY
- :CMODe:THReshold:RFALl:LOWer
- :CMODe:THReshold:RFALl:METHod
- :CMODe:THReshold:RFALl:PAM:ASLevels
- :CMODe:THReshold:RFALl:PAM:PAMLevel:LEVel
- :CMODe:THReshold:RFALl:PLOWer
- :CMODe:THReshold:RFALl:PUPPer
- :CMODe:THReshold:RFALl:TOP
- :CMODe:THReshold:RFALl:TRACking
- :CMODe:THReshold:RFALl:UPPer

## Command Syntax

    :CMODeN:THReshold:GENeral:LOWer <amplitude>

<amplitude> is a double.

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

## Query Syntax

    :CMODeN:THReshold:GENeral:LOWer?

## Description

Sets or queries the lower threshold-definition level. This value is used when making measurements with custom threshold definitions that are based on absolute amplitude. When custom threshold definitions are based on percent, use the `:CMODe:THReshold:GENeral:PLOWer` command.

Use the `:CMODe:THReshold:GENeral:METHod` command to set waveform threshold levels to standard percentages or custom definitions.

Use the `:CMODe:THReshold:GENeral:UPPer` command to enter a upper threshold level. Use the `:CMODe:THReshold:GENeral:MIDDle` command to enter a middle threshold level.

## Example Command Sequence

    :CMODe3_1:THReshold:GENeral:TRACking OFF
    :CMODe3_1:THReshold:GENeral:METHod ABSolute
    :CMODe3_1:THReshold:GENeral:UPPer 125E-3
    :CMODe3_1:THReshold:GENeral:MIDDle 0E0
    :CMODe3_1:THReshold:GENeral:LOWer -125E-3