# :MEASure:JITTer:JITTer:RJComp

Jitter Setup Commands

- :MEASure:JITTer:BSCale
- :MEASure:JITTer:GSCale
- :MEASure:JITTer:JITTer:ANALysis
- :MEASure:JITTer:JITTer:DIMensions
- :MEASure:JITTer:JITTer:DMAXimized
- :MEASure:JITTer:JITTer:EDGE
- :MEASure:JITTer:JITTer:EOPening
- :MEASure:JITTer:JITTer:EOPening:PROBability
- :MEASure:JITTer:JITTer:FLAG
- :MEASure:JITTer:JITTer:FLEad
- :MEASure:JITTer:JITTer:MODE
- :MEASure:JITTer:JITTer:NUINtervals
- :MEASure:JITTer:JITTer:PTYPe
- :MEASure:JITTer:JITTer:RJBandwidth
- :MEASure:JITTer:JITTer:RJComp
- :MEASure:JITTer:JITTer:RJCResult?
- :MEASure:JITTer:JITTer:RJCValue
- :MEASure:JITTer:JITTer:RJSTabilize
- :MEASure:JITTer:JITTer:RJSValue
- :MEASure:JITTer:JITTer:SMEThod
- :MEASure:JITTer:JITTer:TJBer
- :MEASure:JITTer:JITTer:UNITs
- :MEASure:JITTer:SOURce

## Command Syntax

    :MEASure:JITTerN:JITTer:RJComp {OFF | CUSTom | AUTomatic}

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Syntax

    :MEASure:JITTerN:JITTer:RJComp?

## Description

This command selects the RJ compensation option:

OFF
  Disables RJ compensation.
CUSTom
  Enables a user-defined value for RJ compensation.
  If there are known contributors to random jitter, you can use RJ Compensation to compensate or remove jitter from the measurement results.
  Use the `:MEASure:JITTer:JITTer:RJCValue` command to specify the appropriate RJ compensation value.
AUTomatic
  Uses the RN compensation values specified by the `:MEASure:JITTer:NOISe:RNComp` command.