# :MEASure:HORizontal:HTIMe:UREFerence:VALue

Hold Time Commands

- :MEASure:HORizontal:HTIMe
- :MEASure:HORizontal:HTIMe:CEDirection
- :MEASure:HORizontal:HTIMe:DEDirection
- :MEASure:HORizontal:HTIMe:FAVorite
- :MEASure:HORizontal:HTIMe:LOCation?
- :MEASure:HORizontal:HTIMe:OCCurrences
- :MEASure:HORizontal:HTIMe:REGion
- :MEASure:HORizontal:HTIMe:SOURce
- :MEASure:HORizontal:HTIMe:STATus?
- :MEASure:HORizontal:HTIMe:STATus:DETails?
- :MEASure:HORizontal:HTIMe:STATus:REASon?
- :MEASure:HORizontal:HTIMe:UREFerence:STATe
- :MEASure:HORizontal:HTIMe:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:HTIMe:UREFerence:VALue <time_location>

<time_location> is a double.

## Query Syntax

    :MEASure:HORizontal:HTIMe:UREFerence:VALue?

## Description

When a user-defined horizontal reference location is enabled (see `:MEASure:HORizontal:HTIMe:UREFerence:STATe`), this command specifies its time location with respect to the trigger (t = 0) location.