# :CGMemory:THReshold:GENeral:HYSTeresis

:CGMemory Threshold Commands

- :CGMemory:TBASe:GENeral:METHod
- :CGMemory:TBASe:RFALl:METHod
- :CGMemory:THReshold:GENeral:AUTO
- :CGMemory:THReshold:GENeral:BASE
- :CGMemory:THReshold:GENeral:HYSTeresis
- :CGMemory:THReshold:GENeral:LOWer
- :CGMemory:THReshold:GENeral:METHod
- :CGMemory:THReshold:GENeral:MIDDle
- :CGMemory:THReshold:GENeral:PLOWer
- :CGMemory:THReshold:GENeral:PMIDdle
- :CGMemory:THReshold:GENeral:PUPPer
- :CGMemory:THReshold:GENeral:STZero
- :CGMemory:THReshold:GENeral:TOP
- :CGMemory:THReshold:GENeral:TRACking
- :CGMemory:THReshold:GENeral:UPPer
- :CGMemory:THReshold:RFALl:BASE
- :CGMemory:THReshold:RFALl:LOWer
- :CGMemory:THReshold:RFALl:METHod
- :CGMemory:THReshold:RFALl:PLOWer
- :CGMemory:THReshold:RFALl:PUPPer
- :CGMemory:THReshold:RFALl:TOP
- :CGMemory:THReshold:RFALl:TRACking
- :CGMemory:THReshold:RFALl:UPPer

## Command Syntax

    :CGMemoryN:THReshold:GENeral:HYSTeresis <plus_or_minus_value>

<plus_or_minus_value> is a double.

Where N identifies one of eight color grade memories. For example, the color grade memory 2 would be identified as :CGMemory2.

## Query Syntax

    :CGMemoryN:THReshold:GENeral:HYSTeresis?

## Description

When the `:CGMemory:THReshold:GENeral:METHod` setting is `HYSTeresis`, this command sets the user-defined ±hysteresis value for the waveform source.

Use the `:CGMemory:THReshold:GENeral:MIDDle` command to enter the center threshold level.

## Example Command Sequence

    :CGMemory2:THReshold:GENeral:TRACking OFF
    :CGMemory2:THReshold:GENeral:METHod HYSTeresis
    :CGMemory2:THReshold:GENeral:HYSTeresis 125E-3
    :CGMemory2:THReshold:GENeral:MIDDle 0E0