# :MEASure:HISTogram{N}:MODE:STATus?

W-Hist Mode Commands

- :MEASure:HISTogram{N}:MODE?
- :MEASure:HISTogram{N}:MODE:LOCation?
- :MEASure:HISTogram{N}:MODE:STATus?
- :MEASure:HISTogram{N}:MODE:STATus:DETails?
- :MEASure:HISTogram{N}:MODE:STATus:REASon?

## Query Syntax

    :MEASure:HISTogram{1:4}:MODE:STATus?

## Query Response

    {CORR | INV | QUES}

CORR
  The measurement result is correct.
INV
  The measurement result is invalid. A question mark (?) is shown in the displayed results table instead of a measurement result.
QUES
  The measurement result is questionable. A question mark (?) is shown in the displayed results table next to the measurement result.

## Description

Queries the status of the MODE measurement. Use the `:MEASure:HISTogram{N}:MODE:STATus:REASon?` child query to determine the reason for an invalid or questionable measurement. Additional information about the failure may be available using the `:MEASure:HISTogram{N}:MODE:STATus:DETails?` child query.

## See Also

- Measurement Errors