# :MEASure:VERTical:PPHRatio:STATus:DETails?

Peak-to-Peak at Hit Ratio Commands

- :MEASure:VERTical:PPHRatio
- :MEASure:VERTical:PPHRatio:FAVorite
- :MEASure:VERTical:PPHRatio:LOCation?
- :MEASure:VERTical:PPHRatio:REGion
- :MEASure:VERTical:PPHRatio:SOURce
- :MEASure:VERTical:PPHRatio:STATus?
- :MEASure:VERTical:PPHRatio:STATus:DETails?
- :MEASure:VERTical:PPHRatio:STATus:REASon?
- :MEASure:VERTical:PPHRatio:THRatio
- :MEASure:VERTical:PPHRatio:UNITs
- :MEASure:VERTical:PPHRatio:UREFerence:STATe
- :MEASure:VERTical:PPHRatio:UREFerence:VALue

## Query Syntax

    :MEASure:VERTical:PPHRatio:STATus:DETails?

## Description

Returns a string that may provide additional details for a failed Peak-Peak at Hit Ratio measurement (`:MEASure:VERTical:PPHRatio`). If the measurement was successful, a null string is returned.

For a basic description of a measurement failure, use the `:MEASure:VERTical:PPHRatio:STATus:REASon?` sibling query. Use the `:MEASure:VERTical:PPHRatio:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors

## Measurement Identification

Avoid subtle programming errors! To ensure that the correct measurement is installed or queried, always explicitly identify a measurement when installing a measurement or querying a measured value, status, or detail. To identify a measurement, specify the measurement's source waveform (`:SOURce` child command). With some measurements, you may also need to specify other identifying values. Generally, when selecting a measurement using Infiniium's GUI, if a dialog appears prompting you to select values, you should explicitly specify these values when remotely identifying the measurement.

For example, to return the status of the `:MEASure:VERTical:PPHRatio` measurement:

    Infiniium.write(':MEASure:VERTical:PPHRatio:SOURce CHAN1_1')
    if Infiniium.query(':MEASure:VERTical:PPHRatio:STATus?') == 'CORR';
        measurement = Infiniium.query(':MEASure:VERTical:PPHRatio?')