# :MEASure:USER:USER{N}:UREFerence:VALue

User-Defined Waveform Measurement Commands

- :MEASure:USER:USER{N}
- :MEASure:USER:USER{N}:ABBReviation?
- :MEASure:USER:USER{N}:CFILe
- :MEASure:USER:USER{N}:CFILe:CLEar
- :MEASure:USER:USER{N}:CFILe:RELoad
- :MEASure:USER:USER{N}:CFLoaded?
- :MEASure:USER:USER{N}:COMMents?
- :MEASure:USER:USER{N}:FAVorite
- :MEASure:USER:USER{N}:LOCation?
- :MEASure:USER:USER{N}:LSTatus?
- :MEASure:USER:USER{N}:LSTatus:REASon?
- :MEASure:USER:USER{N}:NAME?
- :MEASure:USER:USER{N}:REGion
- :MEASure:USER:USER{N}:SOURce{1:2}
- :MEASure:USER:USER{N}:STATus?
- :MEASure:USER:USER{N}:STATus:DETails?
- :MEASure:USER:USER{N}:STATus:REASon?
- :MEASure:USER:USER{N}:UREFerence:STATe
- :MEASure:USER:USER{N}:UREFerence:VALue

## Command Syntax

    :MEASure:USER:USER{1:8}:UREFerence:VALue <time_location>

<time_location> is a double.

## Query Syntax

    :MEASure:USER:USER{1:8}:UREFerence:VALue?

## Description

When a user-defined horizontal reference location is enabled (see `:MEASure:USER:USER{N}:UREFerence:STATe`), this command specifies its time location with respect to the trigger (t = 0) location.