# Noise Measurement Commands

Jitter

- Jitter Setup
- Jitter Measurement Commands
- Jitter Graph Commands
- Noise Setup
- Noise Measurement Commands
- Noise Graph Commands
- Jitter/Noise Advanced Setup

The Noise analysis measurement commands include:

- :MEASure:JITTer:NOISe:COUNt? — Bit Count
- :MEASure:JITTer:NOISe:DI? — DI (δ-δ), Deterministic Interference
- :MEASure:JITTer:NOISe:EHEight? — Eye Height
- :MEASure:JITTer:NOISe:ISI? — ISI (p-p), Inter-Symbol Interference
- :MEASure:JITTer:NOISe:LEVel? — Level
- :MEASure:JITTer:NOISe:PI? — PI (δ-δ), Periodic Interference Delta-Delta
- :MEASure:JITTer:NOISe:PIR? — PI (rms), Periodic Interference RMS
- :MEASure:JITTer:NOISe:RN? — RN (rms), Random Noise RMS
- :MEASure:JITTer:NOISe:SAMPlitude? — Signal Amplitude
- :MEASure:JITTer:NOISe:TI? — TI (1E-XX), Total Interference (p-p)
- :MEASure:JITTer:NOISe:UIS? — Number of Unit Intervals on which noise measurements are based
- :MEASure:JITTer:NOISe:VECLosure? — VEC (1E-XX), Vertical Eye Closure (p-p)