# :CHANnel Calibration Appliance Setup Commands

:CHANnel Calibration Appliance Setup Commands

- :CHANnel:CAPPliance:AMPLitude
- :CHANnel:CAPPliance:DCBias
- :CHANnel:CAPPliance:MODE
- :CHANnel:CAPPliance:STATe?

These commands are available when an Oscilloscope Optimization module is connected to an oscilloscope input channel (for oscilloscope frame adjustment/calibration).

Oscilloscope frame adjustment/calibration is typically performed at a Keysight Service Center using the graphical user interface, so it is unlikely you will ever use these commands.

In order to work properly, the input of the Oscilloscope Optimization module must be connected to AUX OUT.

The Oscilloscope Optimization module should never be connected to CAL OUT.