# :STATus:OVERload:ALL:EVENt?

Operation Status Registers Commands

- :STATus:ADERegister:EVENt?
- :STATus:ADERegister:ENABle
- :STATus:CALibration:EVENt?
- :STATus:CALibration:ENABle
- :STATus:CLIPped:ALL:CONNection:BANK:EVENt?
- :STATus:CLIPped:ALL:CONNection:BANK:ENABle
- :STATus:CLIPped:ALL:CONNection:EVENt?
- :STATus:CLIPped:ALL:CONNection:ENABle
- :STATus:CLIPped:ALL:EVENt?
- :STATus:CLIPped:ALL:ENABle
- :STATus:CLIPped:EVENt?
- :STATus:CLIPped:ENABle
- :STATus:LTESt:EVENt?
- :STATus:LTESt:ENABle
- :STATus:OPERation:EVENt?
- :STATus:OPERation:ENABle
- :STATus:OVERload:ALL:CONNection:BANK:EVENt?
- :STATus:OVERload:ALL:CONNection:BANK:ENABle
- :STATus:OVERload:ALL:CONNection:EVENt?
- :STATus:OVERload:ALL:CONNection:ENABle
- :STATus:OVERload:ALL:EVENt?
- :STATus:OVERload:ALL:ENABle
- :STATus:OVERload:EVENt?
- :STATus:OVERload:ENABle
- :STATus:TRIGger:EVENt?
- :STATus:TRIGger:ENABle

## Query Syntax

    :STATus:OVERload:ALL:EVENt?

## Description

Reads the Overload All register to see which instruments have reported channel overloads since the last time the register was read.

Reading the register once will clear the status for all instruments.

Reporting of event register bits in the status register system is controlled by the mask loaded into the enable register. All true event bits, that are enabled, are logically "OR"ed, which results in setting true bit 13 (OVLD-ALL) of the Operation Status Register.

Overload All Register Commands
Register | Read | Write | Command
--- | --- | --- | ---
Event | ♦ |  | :STATus:OVERload:ALL:EVENt?
Enable (mask) | ♦ | ♦ | :STATus:OVERload:ALL:ENABle

Overload All Register Bits
Bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
Bit Weight | 32768 | 16384 | 8192 | 4096 | 2048 | 1024 | 512 | 256 | 128 | 64 | 32 | 16 | 8 | 4 | 2 | 1
Event Register | — | — | — | — | — | — | — | — | CONN8 | CONN7 | CONN6 | CONN5 | CONN4 | CONN3 | CONN2 | CONN1
Enable Register |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Sets | to Bit 13 (OVLD-ALL) of Operation Status Register

## Bit Definitions

CONN1-CONN8
  A true indicates the instrument on the connection has reported channel overloads since the last time the register was read. If there are fewer than eight instruments/connections, only those bits are used.