# :WAVeform:CLIPped?

:WAVeform General Commands

- :WAVeform:CLIPped?
- :WAVeform:HOLes?
- :WAVeform:SOURce
- :WAVeform:STATus?
- :WAVeform:STATus:DETails?
- :WAVeform:STATus:REASon?

## Query Syntax

    :WAVeform:CLIPped?

## Query Response

    {NONE | CHIG | CLOW | CBOT}

- `NONE` — No clipped
- `CHIGh` — Clipped high
- `CLOW` — Clipped low
- `CBOTh` — Clipped high and low

## Description

Returns whether the waveform data has been vertically clipped. The amplitude of a clipped-high data point is too high to be displayed on the screen. The amplitude of a clipped-low data point is too low to be displayed on the screen.

Clipped data points (high and low) have the value NaN (9.91E+37).

Use the `:SYSTem:AUToscale` command to properly scale the waveform to the display.

Use `:WAVeform:SOURce` to select the source waveform.