# :CALibrate:CALibrator:MODE

:CALibrate Calibrator Commands

- :CALibrate:CALibrator:AOENable
- :CALibrate:CALibrator:DCOFfset
- :CALibrate:CALibrator:ESPeed
- :CALibrate:CALibrator:MODE
- :CALibrate:CALibrator:PWIDth
- :CALibrate:CALibrator:SPULse

## Command Syntax

    :CALibrate:CALibrator:MODE {DC | PCOMp | PCNDc | TOUT | ZERO | ONE | PPOSitive | PNSingle
       | PNEGative | PNSingle | FSYNth | TCLock | DCLock | CSERdes | OMHZ | FMHZ | OHMHz}

## Query Syntax

    :CALibrate:CALibrator:MODE?

## Description

This command selects the output mode:

- `DC` — DC level.

  Use the `:CALibrate:CALibrator:DCOFfset` command to specify the DC voltage level.

- `PCOMp` — Probe Comp.

  Use the `:CALibrate:CALibrator:ESPeed` command to select a slow or fast edge speed.

- `PCNDc` — Probe Comp No DC.

  Use the `:CALibrate:CALibrator:ESPeed` command to select a slow or fast edge speed.

- `TOUT` — Trigger Out.

- `ZERO` — Logic 0.

- `ONE` — Logic 1.

- `PPOSitive` — Pulse Positive.

  Use the `:CALibrate:CALibrator:PWIDth` command to specify the pulse width.

- `PNSingle` — Pulse Positive Single.

  Use the `:CALibrate:CALibrator:PWIDth` command to specify the pulse width.

  Use the `:CALibrate:CALibrator:SPULse` command to output the single pulse.

- `PNEGative` — Pulse Negative.

  Use the `:CALibrate:CALibrator:PWIDth` command to specify the pulse width.

- `PNSingle` — Pulse Negative Single.

  Use the `:CALibrate:CALibrator:PWIDth` command to specify the pulse width.

  Use the `:CALibrate:CALibrator:SPULse` command to output the single pulse.

- `FSYNth` — Frequency Synth.

- `TCLock` — Timebase Clock.

- `DCLock` — Delayed Clock.

- `CSERdes` — Cal Serdes.

- `OMHZ` — 1MHz.

- `FMHZ` — 50MHz.

- `OHMHz` — 100MHz.

For most of the AC signal output modes, you can use the `:CALibrate:CALibrator:AOENable` command to enable the output on the AUX OUT connector as well.. DC levels cannot be enabled on the AUX OUT output.

## Query Response

    {DC | PCOM | PCND | TOUT | ZERO | ONE | PPOS | PNS | PNEG | PNS | FSYN | TCL
       | DCL | CSER | OMHZ | FMHZ | OHMH}