# :STATus:USER:ENABle

Status Byte Registers Commands

- :STATus:LOCal:EVENt?
- :STATus:LOCal:ENABle
- :STATus:MESSage:EVENt?
- :STATus:MESSage:ENABle
- :STATus:TERegister:EVENt?
- :STATus:TERegister:ENABle
- :STATus:USER:EVENt?
- :STATus:USER:ENABle

## Command Syntax

    :STATus:USER:ENABle <mask>

<mask> is an integer, 0 to 65535, representing a mask for the bits in the event register.

## Query Syntax

    :STATus:USER:ENABle?

## Description

Enters a decimal-weighted value in the user enable register that masks the ability to report bits in the user event register.

User Register Commands
Register | Read | Write | Command
--- | --- | --- | ---
Event | ♦ |  | :STATus:USER:EVENt?
Enable (mask) | ♦ | ♦ | :STATus:USER:ENABle

User Status Register Bits
Bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
Bit Weight | 32768 | 16384 | 8192 | 4096 | 2048 | 1024 | 512 | 256 | 128 | 64 | 32 | 16 | 8 | 4 | 2 | 1
Event Register | — | — | — | — | — | — | — | — | — | — | — | CONNection4 | CONNection2 | CONNection3 | CONNection1 | LCL
Enable Register |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Sets | to Bit 1 (USR) of Status Byte Register

## Bit Definitions

LCL
  A true indicates that Infiniium 2026 has transitioned from remote mode to local mode. This status bit originates from the local event register.
CONNection1
  Reserved for future use.
CONNection3
  Reserved for future use.
CONNection2
  Reserved for future use.
CONNection4
  Reserved for future use.