# PAM Measurements

Measurements

- Time Measurements
- Amplitude Measurements
- Clock Measurements
- Data Measurements
- SNDR Measurements
- PAM Measurements
- FFT Measurements
- User-Defined Measurements
- NRZ Eye Measurements
- PAM Eye Measurements
- Mask Test Commands
- Querying Measurement Results and Statistics

These measurements are optimized for PAM signals. If used with an NRZ signal, the low and high level results are reported as levels 0 and 3 while the level 1 and 2 results are not valid.

- PAM Analysis Setup Commands

- :MEASure:PAM:LEVel (Levels)
- :MEASure:PAM:RFTime (Rise/Fall Times)
- :MEASure:PAM:RMS (Levels RMS)