# :LTESt:MTESt:SWAVeform:DIFF{N}:STATe

:LTESt Mask Limit Commands

- :LTESt:MTESt:MRESult{N}:CTYPe
- :LTESt:MTESt:MRESult{N}:CTYPe:UINTervals
- :LTESt:MTESt:MRESult{N}:CTYPe:WAVeforms
- :LTESt:MTESt:MRESult{N}:SOFailure
- :LTESt:MTESt:MRESult{N}:STATe
- :LTESt:MTESt:SIMage:FNAMe
- :LTESt:MTESt:SIMage:FNAMe:AUPDate
- :LTESt:MTESt:SIMage:FNAMe:USTandard
- :LTESt:MTESt:SIMage:FTYPe?
- :LTESt:MTESt:SIMage:IMETadata
- :LTESt:MTESt:SIMage:INVert
- :LTESt:MTESt:SIMage:MONochrome
- :LTESt:MTESt:SIMage:SINClude
- :LTESt:MTESt:SIMage:STATe
- :LTESt:MTESt:SIMage:WINDow
- :LTESt:MTESt:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:MTESt:SWAVeform:CHANnel:FTYPe
- :LTESt:MTESt:SWAVeform:CHANnel{N}:STATe
- :LTESt:MTESt:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:MTESt:SWAVeform:CMODe{N}:FNAMe
- :LTESt:MTESt:SWAVeform:CMODe:FTYPe
- :LTESt:MTESt:SWAVeform:CMODe{N}:STATe
- :LTESt:MTESt:SWAVeform:CMODe{N}:WMEMory
- :LTESt:MTESt:SWAVeform:DIFF{N}:FNAMe
- :LTESt:MTESt:SWAVeform:DIFF:FTYPe
- :LTESt:MTESt:SWAVeform:DIFF{N}:STATe
- :LTESt:MTESt:SWAVeform:DIFF{N}:WMEMory
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:STATe
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:MTESt:SWAVeform:RESet

## Command Syntax

    :LTESt:MTESt:SWAVeform:DIFF{N}:STATe {DISK | MEMory | OFF}

{N} identifies the differential waveform, which must be selected from "<connection1-8>_<ch1,3,5,7>". For example, the differential waveform of connection 4 channels 1 and 2 would be identified as DIFF4_1.

## Query Syntax

    :LTESt:MTESt:SWAVeform:DIFF{N}:STATe?

## Query Response

    {DISK | MEM | OFF}

## Description

Saves a differential waveform to a file after the mask limit test acquires the specified number of failures. Use the `:LTESt:MTESt:SWAVeform:DIFF{N}:FNAMe` command to specify the file name.