# :MEASure:HORizontal:BINTerval:STATus:REASon?

Burst Interval Commands

- :MEASure:HORizontal:BINTerval
- :MEASure:HORizontal:BINTerval:BIDLe
- :MEASure:HORizontal:BINTerval:FAVorite
- :MEASure:HORizontal:BINTerval:LOCation?
- :MEASure:HORizontal:BINTerval:OCCurrences
- :MEASure:HORizontal:BINTerval:REGion
- :MEASure:HORizontal:BINTerval:SOURce
- :MEASure:HORizontal:BINTerval:STATus?
- :MEASure:HORizontal:BINTerval:STATus:DETails?
- :MEASure:HORizontal:BINTerval:STATus:REASon?
- :MEASure:HORizontal:BINTerval:UREFerence:STATe
- :MEASure:HORizontal:BINTerval:UREFerence:VALue

## Query Syntax

    :MEASure:HORizontal:BINTerval:STATus:REASon?

## Query Response

Refer to the table "Common Reasons for INV or QUES Status".

## Description

Returns a string that explains the reason for a failed `:MEASure:HORizontal:BINTerval` measurement. If the measurement was successful, a null string is returned.

Additional information about the failure may be available using the `:MEASure:HORizontal:BINTerval:STATus:DETails?` sibling query. Use the `:MEASure:HORizontal:BINTerval:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors