# :STATus:USER:EVENt?

Status Byte Registers Commands

- :STATus:LOCal:EVENt?
- :STATus:LOCal:ENABle
- :STATus:MESSage:EVENt?
- :STATus:MESSage:ENABle
- :STATus:TERegister:EVENt?
- :STATus:TERegister:ENABle
- :STATus:USER:EVENt?
- :STATus:USER:ENABle

## Query Syntax

    :STATus:USER:EVENt?

## Description

Reads the user event register to determine the status of individual status bits. The decimal-weighted value of the register is returned. The only bit used is bit 0 (LCL), which indicates if Infiniium 2026 has been placed in local mode (exited remote mode). The other 15 bits are reserved.

Reporting of event register bits in the status register system is controlled by the mask loaded into the enable register. All true event bits, that are enabled, are logically "OR"ed, which results in setting true bit 1 (USR) of the Status Byte Register.

User Register Commands
Register | Read | Write | Command
--- | --- | --- | ---
Event | ♦ |  | :STATus:USER:EVENt?
Enable (mask) | ♦ | ♦ | :STATus:USER:ENABle

User Status Register Bits
Bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
Bit Weight | 32768 | 16384 | 8192 | 4096 | 2048 | 1024 | 512 | 256 | 128 | 64 | 32 | 16 | 8 | 4 | 2 | 1
Event Register | — | — | — | — | — | — | — | — | — | — | — | CONNection4 | CONNection2 | CONNection3 | CONNection1 | LCL
Enable Register |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Sets | to Bit 1 (USR) of Status Byte Register

## Bit Definitions

LCL
  A true indicates that Infiniium 2026 has transitioned from remote mode to local mode. This status bit originates from the local event register.
CONNection1
  Reserved for future use.
CONNection3
  Reserved for future use.
CONNection2
  Reserved for future use.
CONNection4
  Reserved for future use.