# :FUNCtion:PARameters:DDEMbed:DRESult

DeEmbed (4 port) Parameters Commands

- :FUNCtion:PARameters:DDEMbed:ALIGn
- :FUNCtion:PARameters:DDEMbed:BANDwidth
- :FUNCtion:PARameters:DDEMbed:BLIMit
- :FUNCtion:PARameters:DDEMbed:BSPan?
- :FUNCtion:PARameters:DDEMbed:CFRequency
- :FUNCtion:PARameters:DDEMbed:DRESult
- :FUNCtion:PARameters:DDEMbed:FNAMe
- :FUNCtion:PARameters:DDEMbed:IMPulse
- :FUNCtion:PARameters:DDEMbed:MEASsim
- :FUNCtion:PARameters:DDEMbed:RCORr
- :FUNCtion:PARameters:DDEMbed:RESolution
- :FUNCtion:PARameters:DDEMbed:SPAN
- :FUNCtion:PARameters:DDEMbed:STEP

## Command Syntax

    :FUNCtionN:PARameters:DDEMbed:DRESult {DIFFerential | CMODe | SPLus | SMINus}

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtionN:PARameters:DDEMbed:DRESult?

## Description

Selects the output type of a 4-Port DeEmbedding operator (`:FUNCtion:FOPerator`). Use the `:FUNCtion:PARameters:DDEMbed:BANDwidth` command to specify the function's bandwidth. Use the `:FUNCtion:PARameters:DDEMbed:BLIMit` command to specify a bandwidth filter. Use the `:FUNCtion:PARameters:DDEMbed:FNAMe` command to open an existing network file that models your test setup.

DIFFerential
  Specifies a differential output signal.
CMODe
  Specifies a common mode output signal.
SPLus
  Specifies a single-ended (+) output signal.
SMINus
  Specifies a single-ended (−) output signal.

## Example Command Sequence

    :FUNCtion2:FOPerator DDEMbed
    :FUNCtion2:PARameters:DDEMbed:FNAMe "C:\Users<user_name>\Documents\Keysight\Infiniium\De-Embedding Networks\DUT_4.tf4"
    :FUNCtion2:PARameters:DDEMbed:DRESult DIFFerential
    :FUNCtion2:COLor TCOLor4
    :FUNCtion2:DISPlay ON
    *OPC?
    …  //  Your code to synchronize execution timing.

## Child Commands

- `:FUNCtion:PARameters:DDEMbed:BANDwidth`
- `:FUNCtion:PARameters:DDEMbed:BLIMit`
- `:FUNCtion:PARameters:DDEMbed:FNAMe`