# Receiver Impedance Setup

The Receiver Impedance Setup dialog box is displayed whenever you click on the impedance symbol in your network setup diagram.

Use this dialog box to enter the impedance values for both the Measurement and Simulation circuits.

To use one value to define both Measurement and Simulation circuits, select Use Single Impedance Value.

The default impedance value is 50 ohms.

To model a pull-up voltage on the receiver, select Pull-Up and enter the voltage value in the Pull-Up Voltage field.

2-Port De-Embedding Receiver Impedance Setup

4-Port De-Embedding Receiver Impedance Setup