# :MEASure:PAM:RFTime:EDIRection

PAM Rise/Fall Times Commands

- :MEASure:PAM:RFTime
- :MEASure:PAM:RFTime:EDIRection
- :MEASure:PAM:RFTime:FAVorite
- :MEASure:PAM:RFTime:LOCation?
- :MEASure:PAM:RFTime:OCCurrences
- :MEASure:PAM:RFTime:REGion
- :MEASure:PAM:RFTime:SOURce
- :MEASure:PAM:RFTime:STATus?
- :MEASure:PAM:RFTime:STATus:DETails?
- :MEASure:PAM:RFTime:STATus:REASon?
- :MEASure:PAM:RFTime:TRANsition
- :MEASure:PAM:RFTime:UREFerence:STATe
- :MEASure:PAM:RFTime:UREFerence:VALue

## Command Syntax

    :MEASure:PAM:RFTime:EDIRection {RISing | FALLing}

## Query Syntax

    :MEASure:PAM:RFTime:EDIRection?

## Description

Selects the edge direction of a PAM signal level-to-level transition (see `:MEASure:PAM:RFTime:TRANsition`) that will be measured when the `:MEASure:PAM:RFTime` parent command is sent.