# :WAVeform CGRade Commands

:WAVeform CGRade Commands

- :WAVeform:CGRade:ASCii:DATA?
- :WAVeform:CGRade:COLumns?
- :WAVeform:CGRade:INTeger:DATA?
- :WAVeform:CGRade:POINts?
- :WAVeform:CGRade:ROWS?
- :WAVeform:CGRade:STATus?
- :WAVeform:CGRade:STATus:REASon?
- :WAVeform:CGRade:UICount?
- :WAVeform:CGRade:WCOunt?
- :WAVeform:CGRade:XINCrement?
- :WAVeform:CGRade:XML:READ?
- :WAVeform:CGRade:XML:WRITe?
- :WAVeform:CGRade:XORigin?
- :WAVeform:CGRade:YINCrement?
- :WAVeform:CGRade:YORigin?

## Eye Format Waveform Data (CGS)

Returns color grade/gray scale database values in ASCII or binary (16-bit integer) format. Color grade/gray scale data is transferred as a two dimensional array consisting of 521 rows by 751 columns for a total number of 391,271 points. This array corresponds to the graticule display, where each point contains a sample hit count. The array is transferred column by column, starting with the lower left corner of the graticule.

The time for any column of data points:
  Xtime = (Xcolumn)(Xincrement) + (Xorigin)
To amplitude for any data point at a given row:
  Yamplitude = (Yrow)(Yincrement) + Yorigin