# :MEASure:DATA:NUINterval:DWMode

N-UI Commands

- :MEASure:DATA:NUINterval
- :MEASure:DATA:NUINterval:DWMode
- :MEASure:DATA:NUINterval:FAVorite
- :MEASure:DATA:NUINterval:LOCation?
- :MEASure:DATA:NUINterval:NDRate
- :MEASure:DATA:NUINterval:NUINtervals
- :MEASure:DATA:NUINterval:REGion
- :MEASure:DATA:NUINterval:SOURce
- :MEASure:DATA:NUINterval:STATus?
- :MEASure:DATA:NUINterval:STATus:DETails?
- :MEASure:DATA:NUINterval:STATus:REASon?
- :MEASure:DATA:NUINterval:UREFerence:STATe
- :MEASure:DATA:NUINterval:UREFerence:VALue

## Command Syntax

    :MEASure:DATA:NUINterval:DWMode {AUTomatic | SAUTomatic}

## Query Syntax

    :MEASure:DATA:NUINterval:DWMode?

## Description

For the N-UI measurement, specifies whether Automatic clock recovery or Semi Automatic clock recovery be performed.

- In Automatic mode, the data rate is found by searching your waveform for the narrowest data pulse. When the Automatic mode has trouble finding the data rate due to excessive high-frequency jitter on the waveform, the Semi Automatic mode can be used.
- In the Semi Automatic mode, Infiniium starts by searching around the data rate that you specify then automatically finds the data rate.

## Example Command Sequence

This sequence sets up the measurement on rising edges only.

    :MEASure:DATA:NUINterval:SOURce CHAN1_1
    :MEASure:DATA:NUINterval:NUINtervals 4
    :MEASure:DATA:NUINterval:DWMode AUTomatic
      //  Perform measurement
    :MEASure:DATA:NUINterval
    :MEASure:DATA:NUINterval?