# Amplitude Measurements

Subtopics

- Amplitude at Lower
- Amplitude at Middle
- Amplitude at Time
- Amplitude at Upper
- Amplitude
- Average
- Carrier Power
- Crossing
- Maximum
- Minimum
- Overshoot
- Peak-Peak Amplitude
- Peak-Peak at Hit Ratio
- Preshoot
- RMS
- Waveform Base
- Waveform Top

## Toolbar Buttons

Amplitude
Peak-Peak Amplitude
Waveform Top
Waveform Base
Maximum
Minimum
RMS

##

Carrier Power
Amplitude at Lower
Amplitude at Middle
Amplitude at Time
Amplitude at Upper
Average
Crossing

##

Overshoot
Preshoot
Peak-Peak at Hit Ratio

## PAM-Compatible Measurements on the Amplitude Toolbar

Some, but not all, of the NRZ measurements listed in the Time and Amplitude tabs of the measurements toolbar can be used on PAM waveforms. The measurements that you can use are shown in the following tables.

### Compatible

- Amplitude at Time
- Average
  (over display or region)
- Maximum
- Minimum
- Peak-Peak Amplitude
- RMS
  (over display or region)

### Compatible
(Depending on Waveform)

- Amplitude
- Amplitude at Lower
- Amplitude at Middle
- Amplitude at Upper
- Average
  (over cycle)
- Overshoot
- Preshoot
- RMS
- Waveform Base
- Waveform Top