# :TRIGger:AUX:LEVel:FIFTy

:TRIGger General Commands

- :TRIGger:AUX:LEVel
- :TRIGger:AUX:LEVel:FIFTy
- :TRIGger:CHANnel:HTHReshold
- :TRIGger:CHANnel:LEVel
- :TRIGger:CHANnel:LEVel:FIFTy
- :TRIGger:CHANnel:LTHReshold
- :TRIGger:FORCe
- :TRIGger:HYSTeresis
- :TRIGger:MODE
- :TRIGger:SWEep

## Command Syntax

    :TRIGger:AUX:LEVel:FIFTy

## Description

Automatically sets the Aux Trig In input's trigger level to 50% of the input signal amplitude.

This is the same a pushing the oscilloscope's front panel Trigger Level knob.

The Aux Trig In input can be selected as the trigger source in the Edge (`EDGE`) trigger mode (`:TRIGger:MODE`).