# :CALibrate:CONNection:VERTical

:CALibrate Connection Commands

- :CALibrate:CONNection:CLOCk
- :CALibrate:CONNection:ENABled
- :CALibrate:CONNection:EXPort
- :CALibrate:CONNection:IMPort
- :CALibrate:CONNection:SKEW:ENABled
- :CALibrate:CONNection:SKEW:STATus?
- :CALibrate:CONNection:SKEW:STATus:DETails?
- :CALibrate:CONNection:SKEW:STATus:DTEMperature?
- :CALibrate:CONNection:SKEW:STATus:TIME?
- :CALibrate:CONNection:STARt
- :CALibrate:CONNection:STATus?
- :CALibrate:CONNection:STATus:DETails?
- :CALibrate:CONNection:STATus:DTEMperature?
- :CALibrate:CONNection:STATus:TIME?
- :CALibrate:CONNection:TIMebase:ENABled
- :CALibrate:CONNection:TIMebase:EXPort
- :CALibrate:CONNection:TIMebase:IMPort
- :CALibrate:CONNection:TIMebase:STARt
- :CALibrate:CONNection:TRIGger:ENABled
- :CALibrate:CONNection:VERTical
- :CALibrate:CONNection:VERTical:STATus?
- :CALibrate:CONNection:VERTical:STATus:DETails?
- :CALibrate:CONNection:VERTical:STATus:DTEMperature?
- :CALibrate:CONNection:VERTical:STATus:TIME?

## Command Syntax

    :CALibrate:CONNectionN:VERTical {ENABled | DISabled}

Where N identifies a specific instrument by connection number and must be selected from {1:8}. For an instrument that occupies multiple connections, use the instrument's left-most connection number to identify the instrument. For two-connection instruments, the connection number would be 1 or 3. For four-connection instruments, the connection number would be 1.

## Query Syntax

    :CALibrate:CONNection{1:8}:VERTical?

## Description

For the indicated connection number (instrument), enables or disables the vertical calibration. To perform this calibration along with all other selected calibrations for the indicated connection number, use the `:CALibrate:CONNection:STARt` command. To select all calibrations for the indicated connection number, use the `:CALibrate:CONNection:ENABled` command. These commands affect the Calibration dialog box indicators.

ENABled
  Selects the calibration.
DISabled
  Prevents the calibration.

Use the child queries listed in the following table to return details about the current calibration.

Status String Child Queries
Status String | Child Query to Send
--- | ---
State of Calibration | `:CALibrate:CONNection:VERTical:STATus?`
Time of last calibration, Time change since last calibration, and Temperature change since last calibration | `:CALibrate:CONNection:VERTical:STATus:DETails?`
Change in temperature | `:CALibrate:CONNection:VERTical:STATus:DTEMperature?`
Change in Time | `:CALibrate:CONNection:VERTical:STATus:TIME?`

## Query Response

    {ENAB | DIS | PART}

ENAB
  Indicates that all vertical calibrations for the indicated connection number are selected.
DIS
  Indicates that all vertical calibrations for the indicated connection number are disabled.
PART
  Indicates that some vertical calibrations for the indicated connection number are selected and some are deselected.

## Child Commands

- `:CALibrate:CONNection:VERTical:STATus?` queries the measurement status.
- `:CALibrate:CONNection:VERTical:STATus:DETails?`
- `:CALibrate:CONNection:VERTical:STATus:DTEMperature?`
- `:CALibrate:CONNection:VERTical:STATus:TIME?`