# :LTESt:MEASure:SIMage:STATe

:LTESt Measurement Screen Image Commands

- :LTESt:MEASure:SIMage:FNAMe
- :LTESt:MEASure:SIMage:FNAMe:AUPDate
- :LTESt:MEASure:SIMage:FNAMe:USTandard
- :LTESt:MEASure:SIMage:FTYPe?
- :LTESt:MEASure:SIMage:IMETadata
- :LTESt:MEASure:SIMage:INVert
- :LTESt:MEASure:SIMage:MONochrome
- :LTESt:MEASure:SIMage:SINClude
- :LTESt:MEASure:SIMage:STATe
- :LTESt:MEASure:SIMage:WINDow

## Command Syntax

    :LTESt:MEASure:SIMage:STATe {ON | OFF | 1 | 0}

## Query Syntax

    :LTESt:MEASure:SIMage:STATe?

## Query Response

    {1 | 0}

## Description

Selects to save a screen image to a file after the specified number of measurement failures stops the limit test.

Information on identifying the measurement is found in the introduction to the limit test programming subsystem. Use the commands shown in the following table to configure the output file.

Commands to Configure the Output
Task | Command
--- | ---
Enter the filename and path | `:LTESt:MEASure:SIMage:FNAMe`
Enter the graphics file type | `:LTESt:MEASure:SIMage:FTYPe?`
Select portion of Infiniium display to capture | `:LTESt:MEASure:SIMage:WINDow`
Include metadata in jpg and tiff files. | `:LTESt:MEASure:SIMage:IMETadata`
Invert background color | `:LTESt:MEASure:SIMage:INVert`
Black and white output | `:LTESt:MEASure:SIMage:MONochrome`
Capture a single waveform among several displayed waveforms | `:LTESt:MEASure:SIMage:SINClude`