# :MEASure:HORizontal:TVOLt:YVALue

Time-at-Amplitude Commands

- :MEASure:HORizontal:TVOLt
- :MEASure:HORizontal:TVOLt:EDIRection
- :MEASure:HORizontal:TVOLt:ENUMber
- :MEASure:HORizontal:TVOLt:FAVorite
- :MEASure:HORizontal:TVOLt:LOCation?
- :MEASure:HORizontal:TVOLt:REGion
- :MEASure:HORizontal:TVOLt:SOURce
- :MEASure:HORizontal:TVOLt:STATus?
- :MEASure:HORizontal:TVOLt:STATus:DETails?
- :MEASure:HORizontal:TVOLt:STATus:REASon?
- :MEASure:HORizontal:TVOLt:YVALue
- :MEASure:HORizontal:TVOLt:UREFerence:STATe
- :MEASure:HORizontal:TVOLt:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:TVOLt:YVALue  <amplitude>

<amplitude> is a double.

## Query Syntax

    :MEASure:HORizontal:TVOLt:YVALue?

## Description

For the Time-at-Amplitude measurement, specifies the amplitude value at which to perform the measurement. To specify the edge direction, use the `:MEASure:HORizontal:TVOLt:EDIRection` command. To specify the edge number, use the `:MEASure:HORizontal:TVOLt:ENUMber` command.

## Example Command Sequence

    :MEASure:HORizontal:TVOLt:SOURce CHAN1_1
    :MEASure:HORizontal:TVOLt:EDIRection RISing
    :MEASure:HORizontal:TVOLt:ENUMber 1
    :MEASure:HORizontal:TVOLt:YVALue 100E-03
    :MEASure:HORizontal:TVOLt
    :MEASure:HORizontal:TVOLt?