# :CGMemory:THReshold:GENeral:MIDDle

:CGMemory Threshold Commands

- :CGMemory:TBASe:GENeral:METHod
- :CGMemory:TBASe:RFALl:METHod
- :CGMemory:THReshold:GENeral:AUTO
- :CGMemory:THReshold:GENeral:BASE
- :CGMemory:THReshold:GENeral:HYSTeresis
- :CGMemory:THReshold:GENeral:LOWer
- :CGMemory:THReshold:GENeral:METHod
- :CGMemory:THReshold:GENeral:MIDDle
- :CGMemory:THReshold:GENeral:PLOWer
- :CGMemory:THReshold:GENeral:PMIDdle
- :CGMemory:THReshold:GENeral:PUPPer
- :CGMemory:THReshold:GENeral:STZero
- :CGMemory:THReshold:GENeral:TOP
- :CGMemory:THReshold:GENeral:TRACking
- :CGMemory:THReshold:GENeral:UPPer
- :CGMemory:THReshold:RFALl:BASE
- :CGMemory:THReshold:RFALl:LOWer
- :CGMemory:THReshold:RFALl:METHod
- :CGMemory:THReshold:RFALl:PLOWer
- :CGMemory:THReshold:RFALl:PUPPer
- :CGMemory:THReshold:RFALl:TOP
- :CGMemory:THReshold:RFALl:TRACking
- :CGMemory:THReshold:RFALl:UPPer

## Command Syntax

    :CGMemoryN:THReshold:GENeral:MIDDle <amplitude>

<amplitude> is a double.

Where N identifies one of eight color grade memories. For example, the color grade memory 2 would be identified as :CGMemory2.

## Query Syntax

    :CGMemoryN:THReshold:GENeral:MIDDle?

## Description

Sets or queries the middle threshold-definition level. This value is used when making measurements with custom threshold definitions that are based on absolute amplitude. When custom threshold definitions are based on percent, use the `:CGMemory:THReshold:GENeral:PMIDdle` command.

Use the `:CGMemory:THReshold:GENeral:METHod` command to set waveform threshold levels to standard percentages or custom definitions.

Use the `:CGMemory:THReshold:GENeral:UPPer` command to enter a upper threshold level. Use the `:CGMemory:THReshold:GENeral:LOWer` command to enter a lower threshold level.

## Example Command Sequence

    :CGMemory6:THReshold:GENeral:TRACking OFF
    :CGMemory6:THReshold:GENeral:METHod ABSolute
    :CGMemory6:THReshold:GENeral:UPPer 125E-3
    :CGMemory6:THReshold:GENeral:MIDDle 0E0
    :CGMemory6:THReshold:GENeral:LOWer -125E-3