# :CALibrate:CONNection:STATus:DTEMperature?

:CALibrate Connection Commands

- :CALibrate:CONNection:CLOCk
- :CALibrate:CONNection:ENABled
- :CALibrate:CONNection:EXPort
- :CALibrate:CONNection:IMPort
- :CALibrate:CONNection:SKEW:ENABled
- :CALibrate:CONNection:SKEW:STATus?
- :CALibrate:CONNection:SKEW:STATus:DETails?
- :CALibrate:CONNection:SKEW:STATus:DTEMperature?
- :CALibrate:CONNection:SKEW:STATus:TIME?
- :CALibrate:CONNection:STARt
- :CALibrate:CONNection:STATus?
- :CALibrate:CONNection:STATus:DETails?
- :CALibrate:CONNection:STATus:DTEMperature?
- :CALibrate:CONNection:STATus:TIME?
- :CALibrate:CONNection:TIMebase:ENABled
- :CALibrate:CONNection:TIMebase:EXPort
- :CALibrate:CONNection:TIMebase:IMPort
- :CALibrate:CONNection:TIMebase:STARt
- :CALibrate:CONNection:TRIGger:ENABled
- :CALibrate:CONNection:VERTical
- :CALibrate:CONNection:VERTical:STATus?
- :CALibrate:CONNection:VERTical:STATus:DETails?
- :CALibrate:CONNection:VERTical:STATus:DTEMperature?
- :CALibrate:CONNection:VERTical:STATus:TIME?

## Query Syntax

    :CALibrate:CONNectionN:STATus:DTEMperature?

Where N identifies a specific instrument by connection number and must be selected from {1:8}. For an instrument that occupies multiple connections, use the instrument's left-most connection number to identify the instrument. For two-connection instruments, the connection number would be 1 or 3. For four-connection instruments, the connection number would be 1.

## Description

Queries the change in the instrument's temperature from the time when the last vertical, precision timebase, or clock recovery calibration was performed on the indicated connection number. If a calibration has not yet been performed, a value of NaA (9.91E+37) is returned. A calibration should be performed if the change in temperature exceeds ±5°C.

## Example Returned Status

    -6.10

## Parent Command

- `:CALibrate:CONNection:STATus?`