# :CGMemory:THReshold:GENeral:TRACking

:CGMemory Threshold Commands

- :CGMemory:TBASe:GENeral:METHod
- :CGMemory:TBASe:RFALl:METHod
- :CGMemory:THReshold:GENeral:AUTO
- :CGMemory:THReshold:GENeral:BASE
- :CGMemory:THReshold:GENeral:HYSTeresis
- :CGMemory:THReshold:GENeral:LOWer
- :CGMemory:THReshold:GENeral:METHod
- :CGMemory:THReshold:GENeral:MIDDle
- :CGMemory:THReshold:GENeral:PLOWer
- :CGMemory:THReshold:GENeral:PMIDdle
- :CGMemory:THReshold:GENeral:PUPPer
- :CGMemory:THReshold:GENeral:STZero
- :CGMemory:THReshold:GENeral:TOP
- :CGMemory:THReshold:GENeral:TRACking
- :CGMemory:THReshold:GENeral:UPPer
- :CGMemory:THReshold:RFALl:BASE
- :CGMemory:THReshold:RFALl:LOWer
- :CGMemory:THReshold:RFALl:METHod
- :CGMemory:THReshold:RFALl:PLOWer
- :CGMemory:THReshold:RFALl:PUPPer
- :CGMemory:THReshold:RFALl:TOP
- :CGMemory:THReshold:RFALl:TRACking
- :CGMemory:THReshold:RFALl:UPPer

## Command Syntax

    :CGMemoryN:THReshold:GENeral:TRACking  {{ON | 1} | {OFF | 0}}

Where N identifies one of eight color grade memories. For example, the color grade memory 2 would be identified as :CGMemory2.

## Query Syntax

    :CGMemoryN:THReshold:GENeral:TRACking?

## Query Response

    {1 | 0}

## Description

Specifies whether a signal tracks the global threshold definition or uses its own threshold definition.

The global threshold definition is set using the `:MEASure:THReshold:GENeral` commands (see Threshold Configuration Commands).

## Example Command Sequence

    :CGMemory2:THReshold:GENeral:TRACking OFF
    :CGMemory2:THReshold:GENeral:METHod ABSolute
    :CGMemory2:THReshold:GENeral:UPPer 125E-3
    :CGMemory2:THReshold:GENeral:MIDDle 0E0
    :CGMemory2:THReshold:GENeral:LOWer -125E-3