# :MEASure:VERTical:VAVerage:EDIRection

Average Commands

- :MEASure:VERTical:VAVerage
- :MEASure:VERTical:VAVerage:AREA
- :MEASure:VERTical:VAVerage:EDIRection
- :MEASure:VERTical:VAVerage:FAVorite
- :MEASure:VERTical:VAVerage:LOCation?
- :MEASure:VERTical:VAVerage:REGion
- :MEASure:VERTical:VAVerage:SOURce
- :MEASure:VERTical:VAVerage:STATus?
- :MEASure:VERTical:VAVerage:STATus:DETails?
- :MEASure:VERTical:VAVerage:STATus:REASon?
- :MEASure:VERTical:VAVerage:UREFerence:STATe
- :MEASure:VERTical:VAVerage:UREFerence:VALue

## Command Syntax

    :MEASure:VERTical:VAVerage:EDIRection  {RISing | FALLing}

## Query Syntax

    :MEASure:VERTical:VAVerage:EDIRection?

## Description

For the Average amplitude measurement, when the selected area is a single cycle:

- `RISing` or `FALLing` — the cycle beginning with this edge that is nearest to the timebase reference is the cycle to measure.