# :CALibrate:CHANnel:STATus:DETails?

:CALibrate Channel Commands

- :CALibrate:CHANnel:ENABled
- :CALibrate:CHANnel:NOISe?
- :CALibrate:CHANnel:STATus?
- :CALibrate:CHANnel:STATus:DETails?
- :CALibrate:CHANnel:STATus:DTEMperature?
- :CALibrate:CHANnel:STATus:TIME?

## Query Syntax

    :CALibrate:CHANnelN:STATus:DETails?

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, `CHANnel3`.

## Description

Queries a string of status details for the current channel calibration. The following is an example of a typical returned string:

    Time of last Calibration: 10/23/2012 11:52:00,Elapsed Calibration Time: 3 hours 2 minutes,Temperature Change: 1.24 C"

If a calibration is recommended, the following text is placed at the beginning of the above string:

    "Requires Clock Recovery Calibration, …"

If a calibration has not yet been performed, the following string is returned:

    "This calibration has never been performed in this instrument."

## Example Returned Status String

    "Elapsed cal time has exceeded 10 hours.,Time of last Calibration: 09/20/2012 15:11:05,Elapsed Calibration Time: 26 days,Temperature Change: 2.58 C"

## Parent Command

- `:CALibrate:CHANnel:STATus?`