# :FUNCtion:PARameters:DDEMbed:IMPulse

DeEmbed (4 port) Parameters Commands

- :FUNCtion:PARameters:DDEMbed:ALIGn
- :FUNCtion:PARameters:DDEMbed:BANDwidth
- :FUNCtion:PARameters:DDEMbed:BLIMit
- :FUNCtion:PARameters:DDEMbed:BSPan?
- :FUNCtion:PARameters:DDEMbed:CFRequency
- :FUNCtion:PARameters:DDEMbed:DRESult
- :FUNCtion:PARameters:DDEMbed:FNAMe
- :FUNCtion:PARameters:DDEMbed:IMPulse
- :FUNCtion:PARameters:DDEMbed:MEASsim
- :FUNCtion:PARameters:DDEMbed:RCORr
- :FUNCtion:PARameters:DDEMbed:RESolution
- :FUNCtion:PARameters:DDEMbed:SPAN
- :FUNCtion:PARameters:DDEMbed:STEP

## Command Syntax

    :FUNCtionN:PARameters:DDEMbed:IMPulse {ON | OFF | 1 | 0}

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtion{1:64}:PARameters:DDEMbed:IMPulse?

## Query Response

    {1 | 0}

## Description

For an 4-Port DeEmbedding operator (`:FUNCtion:FOPerator`), this command turns on and off the Show Impulse Response option. When selected (on), the selected network file is automatically loaded into the S-Parameter/Transfer Function Viewer and an impulse response chart is added if the parameters can be determined; otherwise, you can add the chart by selecting the proper parameters. See :NETWorks:TRACe General Commands.