# :MEASure:PAM:EYE:TIME:UNITs

PAM Analysis Setup Commands

- :MEASure:PAM:AMPLitude:UNITs
- :MEASure:PAM:EYE:ELMethod
- :MEASure:PAM:EYE:ESTiming
- :MEASure:PAM:EYE:PPERcent
- :MEASure:PAM:EYE:TIME:LTDefinition
- :MEASure:PAM:EYE:TIME:UNITs

## Command Syntax

    :MEASure:PAM:EYE:TIME:UNITs {SECond | UINTerval}

## Query Syntax

    :MEASure:PAM:EYE:TIME:UNITs?

## Description

Sets the time units for PAM width and skew measurements. The units can be seconds (`SECond`) or unit interval (`UINTerval`). The following measurements are affected by this setting:

- PAM Eye Level Skews (`:MEASure:EYE:PAM:SKEW`)
- PAM Eye Skews (`:MEASure:EYE:PAM:ESKew`)
- PAM Eye Widths (`:MEASure:EYE:PAM:EWIDth`)