# :FUNCtion:PARameters:DEMBed:STEP

DeEmbed (2 port) Parameters Commands

- :FUNCtion:PARameters:DEMBed:ALIGn
- :FUNCtion:PARameters:DEMBed:BANDwidth
- :FUNCtion:PARameters:DEMBed:BLIMit
- :FUNCtion:PARameters:DEMBed:BSPan?
- :FUNCtion:PARameters:DEMBed:CFRequency
- :FUNCtion:PARameters:DEMBed:FNAMe
- :FUNCtion:PARameters:DEMBed:IMPulse
- :FUNCtion:PARameters:DEMBed:MEASsim
- :FUNCtion:PARameters:DEMBed:NGAin
- :FUNCtion:PARameters:DEMBed:RCORr
- :FUNCtion:PARameters:DEMBed:RESolution
- :FUNCtion:PARameters:DEMBed:SPAN
- :FUNCtion:PARameters:DEMBed:STEP

## Command Syntax

    :FUNCtionN:PARameters:DEMBed:STEP {ON | OFF | 1 | 0}

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtion{1:64}:PARameters:DEMBed:STEP?

## Query Response

    {1 | 0}

## Description

For a 2-Port DeEmbedding operator (`:FUNCtion:FOPerator`), this command turns on and off the Show Step Response option. When selected (on), the selected network file is automatically loaded into the S-Parameter/Transfer Function Viewer and a step response chart is added if the parameters can be determined; otherwise, you can add the chart by selecting the proper parameters. See :NETWorks:TRACe General Commands.