# :WMEMory:DSTatus?

:WMEMory General Commands

- :WMEMory:CLEar
- :WMEMory:COLor
- :WMEMory:CWINdow
- :WMEMory:DISPlay
- :WMEMory:DSTatus?
- :WMEMory:DSTatus:REASon?
- :WMEMory:INTerpolate:FACTor
- :WMEMory:INTerpolate:METHod
- :WMEMory:INTerpolate:STATus?
- :WMEMory:INTerpolate:STATus:REASon?
- :WMEMory:PATTern:FILE:GCODe
- :WMEMory:PATTern:FILE:NAME
- :WMEMory:PATTern:FILE:RELoad
- :WMEMory:PATTern:INVert
- :WMEMory:PATTern:KPATtern
- :WMEMory:PATTern:MODE
- :WMEMory:SIGNal:TYPE
- :WMEMory:STATus?
- :WMEMory:TTIMebase
- :WMEMory:UNAMe
- :WMEMory:UNAMe:UFName

## Query Syntax

    :WMEMoryN:DSTatus?

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

## Query Response

    {CORR | INV}

## Description

Returns the status of the specified waveform memory. Up to eight memories are available. To query the reason for the current state of the memory, use the `:WMEMory:DSTatus:REASon?` query. The following responses can be returned:

`CORR`
  The memory location contains waveform data. To clear memory, use the `:WMEMory:CLEar` command.
`INV`
  The memory location does not contain waveform data.