# *TRG (Trigger)

Common Commands

- *CLS (Clear Status)
- *ESE (Event Status Enable)
- *ESR? (Event Status Register)
- *IDN? (Identification Number)
- *OPC (Operation Complete)
- *OPT? (Option)
- *RST (Reset)
- *SRE (Service Request Enable)
- *STB? (Status Byte)
- *TRG (Trigger)
- *TST? (Hardware Self Tests)
- *WAI (Wait-to-Continue)

## Command Syntax

    *TRG

## Description

Acquires data for the active waveform display, if the trigger conditions are met, according to the current settings. The `*TRG` common command has the same effect as the `:ACQuire:RUN` command.