# :WMEMory:EYE:CWINdow

:WMEMory EYE Commands

- :WMEMory EYE Commands
- :WMEMory:EYE:BITS
- :WMEMory:EYE:CCOunt
- :WMEMory:EYE:CURSor
- :WMEMory:EYE:CWINdow
- :WMEMory:EYE:DISPlay
- :WMEMory:EYE:PATTern
- :WMEMory:EYE:UIXPosition
- :WMEMory:EYE:UIXRange
- :WMEMory:EYE:UUNits
- :WMEMory:EYE:WINDow:COPY
- :WMEMory:EYE:WINDow:LEFT
- :WMEMory:EYE:WINDow:METHod
- :WMEMory:EYE:WINDow:RIGHt
- :WMEMory:EYE:WINDow:TRACking
- :WMEMory:EYE:WINDow:WIDTh
- :WMEMory:EYE:XPOSition
- :WMEMory:EYE:XSCale

## Command Syntax

    :WMEMoryN:EYE:CWINdow TIME{1:4}

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

## Query Syntax

    :WMEMoryN:EYE:CWINdow?

## Description

The `:WMEMory{1:8}:EYE:CWINdow` command allows you to assign a waveform memory's real-time eye waveform to a Waveform content window.

Command Arguments and Content Windows
Argument | Displayed Waveform Content Window | Number of Available Windows | Scale Units
--- | --- | --- | ---
Programmatically | Via Front Panel
TIME{1:4} | Waveform | 4 | 4 | Y-Axis: Volts or Watts (linear scale) X-Axis: seconds