# :CALibrate:CONTinue

:CALibrate Commands

- :CALibrate Subsystem
- :CALibrate:CANCel
- :CALibrate:CONTinue
- :CALibrate:SDONe?
- :CALibrate Calibrator Commands
- :CALibrate Connection Commands
- :CALibrate Channel Commands
- :CALibrate Probe Commands

## Command Syntax

    :CALibrate:CONTinue

## Description

Continues all calibrations that are in process. As a calibration progresses, message or decision dialogs often appear. For example, the user might be instructed to disconnect any front-panel inputs to an instrument. This command is equivalent to clicking the dialog's Next or Done button. Use the `:CALibrate:CANCel` command for an equivalent of the Cancel button. Use the `:CALibrate:SDONe?` command to pause your application until the user clicks a button and to determine the which button was pressed.

Use an `*OPC (Operation Complete)` query to pause program execution while waiting for this command to complete.

## Example Command Sequence

The following commands are used for a typical vertical calibration.

    :CALibrate:CONNection3:STARt
    :CALibrate:SDONe?
    :CALibrate:CONTinue    //  Dismiss the begin notice calibration dialog box
    :CALibrate:SDONe?
    :CALibrate:CONTinue    //  Dismiss the disconnect notice dialog box
    :CALibrate:SDONe?
    :CALibrate:CONTinue    //  Dismiss calibration complete dialog box
    *OPC?