# :MEASure:HORizontal:TEDGe:NUMBer

Time-at-Edge Commands

- :MEASure:HORizontal:TEDGe
- :MEASure:HORizontal:TEDGe:EDIRection
- :MEASure:HORizontal:TEDGe:FAVorite
- :MEASure:HORizontal:TEDGe:LOCation?
- :MEASure:HORizontal:TEDGe:NUMBer
- :MEASure:HORizontal:TEDGe:REGion
- :MEASure:HORizontal:TEDGe:SOURce
- :MEASure:HORizontal:TEDGe:STATus?
- :MEASure:HORizontal:TEDGe:STATus:DETails?
- :MEASure:HORizontal:TEDGe:STATus:REASon?
- :MEASure:HORizontal:TEDGe:THReshold
- :MEASure:HORizontal:TEDGe:UREFerence:STATe
- :MEASure:HORizontal:TEDGe:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:TEDGe:NUMBer <edge_number>

<edge_number> is an int.

## Query Syntax

    :MEASure:HORizontal:TEDGe:NUMBer?

## Description

For the Time-at-Edge measurement, specifies the edge number used to identify the waveform's edge. To specify the edge threshold, use the `:MEASure:HORizontal:TEDGe:THReshold` command. To specify the edge direction, use the `:MEASure:HORizontal:TEDGe:EDIRection` command.

## Example Command Sequence

    :MEASure:HORizontal:TEDGe:SOURce CHAN2_2
    :MEASure:HORizontal:TEDGe:EDIRection RISing
    :MEASure:HORizontal:TEDGe:NUMBer 2
    :MEASure:HORizontal:TEDGe:THReshold MIDDle
    :MEASure:HORizontal:TEDGe
    :MEASure:HORizontal:TEDGe?