# :DIFF:EYE:WINDow:WIDTh

:DIFF EYE Commands

- :DIFF EYE Commands
- :DIFF:EYE:BITS
- :DIFF:EYE:CCOunt
- :DIFF:EYE:CURSor
- :DIFF:EYE:CWINdow
- :DIFF:EYE:DISPlay
- :DIFF:EYE:PATTern
- :DIFF:EYE:UIXPosition
- :DIFF:EYE:UIXRange
- :DIFF:EYE:UUNits
- :DIFF:EYE:XPOSition
- :DIFF:EYE:XSCale

## Command Syntax

    :DIFFN:EYE:WINDow:WIDTh<percent>

Where N identifies a specific differential waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 differential waveform 3 (from the pairing of channels 3 and 4) is `DIFF5_3`.

<percent> is a double.

## Query Syntax

    :DIFFN:EYE:WINDow:WIDTh?

## Description

When the "At Clock Time" eye window determination method is selected (see `:DIFF:EYE:WINDow:METHod`), this command specifies the UI percentage width about the recovered clock location to use as the eye window. A zero percent for this setting means only the recovered clock location is used.

This command is equivalent to the settings in the Eye tab of the Configure Measurements dialog box.