# :MEASure:PAM:EYE:ELMethod

PAM Analysis Setup Commands

- :MEASure:PAM:AMPLitude:UNITs
- :MEASure:PAM:EYE:ELMethod
- :MEASure:PAM:EYE:ESTiming
- :MEASure:PAM:EYE:PPERcent
- :MEASure:PAM:EYE:TIME:LTDefinition
- :MEASure:PAM:EYE:TIME:UNITs

## Command Syntax

    :MEASure:PAM:EYE:ELMethod {MEWidth | MEHeight}

## Description

Selects the basis for determining the location of an eye's center on the waveform. This setting affects all PAM eye measurements. It does not affect PAM waveform measurements.

Arguments | Description
--- | ---
MEWidth | The eye's center is located at the eye's maximum width midway between the eye's inside left and right edges. This is the default setting.
MEHeight | The eye's center is located at the eye's maximum height midway between the eye's inside top and bottom edges.