# :CMODe:YSCale:FINE

:CMODe Scaling Commands

- :CMODe:YBOTtom?
- :CMODe:YOFFset
- :CMODe:YRANge
- :CMODe:YSCale
- :CMODe:YSCale:FINE
- :CMODe:YTOP?
- :CMODe:YUNits

## Command Syntax

    :CMODeN:YSCale:FINE {{OFF | 0} | {ON | 1}}

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

## Query Syntax

    :CMODeN:YSCale:FINE?

## Query Response

    {0 | 1}

## Description

Enables or disables fine adjustment of the vertical scale.

When OFF (coarse adjustment), the vertical scale is adjusted in a 1-2-5 sequence.

When ON (fine adjustment), the vertical scale is adjusted in smaller, evenly spaced increments.