# :FUNCtion:PARameters:CTLequalizer:TFUNction

CTLE Parameters Commands

- :FUNCtion:PARameters:CTLequalizer:ACGain
- :FUNCtion:PARameters:CTLequalizer:BANDwidth
- :FUNCtion:PARameters:CTLequalizer:BWMode
- :FUNCtion:PARameters:CTLequalizer:DBACgain
- :FUNCtion:PARameters:CTLequalizer:DBGain
- :FUNCtion:PARameters:CTLequalizer:DEFinition
- :FUNCtion:PARameters:CTLequalizer:FZP
- :FUNCtion:PARameters:CTLequalizer:GAIN
- :FUNCtion:PARameters:CTLequalizer:GDC
- :FUNCtion:PARameters:CTLequalizer:IMPulse
- :FUNCtion:PARameters:CTLequalizer:POLE
- :FUNCtion:PARameters:CTLequalizer:PRESets
- :FUNCtion:PARameters:CTLequalizer:PRESets:SELections?
- :FUNCtion:PARameters:CTLequalizer:STEP
- :FUNCtion:PARameters:CTLequalizer:TFUNction
- :FUNCtion:PARameters:CTLequalizer:ZERO

## Command Syntax

    :FUNCtionN:PARameters:CTLequalizer:TFUNction {ON | OFF | 1 | 0}

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtion{1:64}:PARameters:CTLequalizer:TFUNction?

## Query Response

    {1 | 0}

## Description

For the Continuous Time Linear Equalizer (CTLE) operator (`:FUNCtion:FOPerator`), this command turns on and off the Show Transfer Function option. When selected (on), the network is automatically loaded into the S-Parameter/Transfer Function Viewer and a frequency-magnitude chart is added.