# :LTESt:ACQuire:SWAVeform:CMODe{N}:STATe

:LTESt Acquisition Commands

- :LTESt:ACQuire:CTYPe
- :LTESt:ACQuire:CTYPe:SAMPles
- :LTESt:ACQuire:CTYPe:WAVeforms
- :LTESt:ACQuire:SIMage:FNAMe
- :LTESt:ACQuire:SIMage:FNAMe:AUPDate
- :LTESt:ACQuire:SIMage:FNAMe:USTandard
- :LTESt:ACQuire:SIMage:FTYPe?
- :LTESt:ACQuire:SIMage:IMETadata
- :LTESt:ACQuire:SIMage:INVert
- :LTESt:ACQuire:SIMage:MONochrome
- :LTESt:ACQuire:SIMage:SINClude
- :LTESt:ACQuire:SIMage:STATe
- :LTESt:ACQuire:SIMage:WINDow
- :LTESt:ACQuire:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CHANnel:FTYPe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:CMODe{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CMODe:FTYPe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:STATe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:WMEMory WMEMory{1:8}
- :LTESt:ACQuire:SWAVeform:DIFF{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:DIFF:FTYPe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:STATe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:STATe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:RESet

## Command Syntax

    :LTESt:ACQuire:SWAVeform:CMODeN:STATe {DISK | MEMory | OFF}

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

## Query Syntax

    :LTESt:ACQuire:SWAVeform:CMODeN:STATe?

## Query Response

    {DISK | MEM | OFF}

## Description

Selects to save a common-mode waveforms to a file or memory after the limit test acquires the specified number of waveforms, samples, or patterns. Use the `:LTESt:ACQuire:CTYPe` command and its child commands to specify the test conditions required to end the test. To enable or disable acquisition limit tests, use the `:LTESt:ACQuire:STATe` command. The following command arguments are available:

DISK
  Saves the waveform to a file. Use the `:LTESt:ACQuire:SWAVeform:CMODe{N}:FNAMe` command to specify the file name.
MEMory
  Saves the waveform to a memory location. Use the `:LTESt:ACQuire:SWAVeform:CMODe{N}:WMEMory WMEMory{1:8}` command to specify the memory location.
OFF
  Turns off the saving of a common-mode waveform.