# :CALibrate:CALibrator:AOENable

:CALibrate Calibrator Commands

- :CALibrate:CALibrator:AOENable
- :CALibrate:CALibrator:DCOFfset
- :CALibrate:CALibrator:ESPeed
- :CALibrate:CALibrator:MODE
- :CALibrate:CALibrator:PWIDth
- :CALibrate:CALibrator:SPULse

## Command Syntax

    :CALibrate:CALibrator:AOENable {{OFF | 0} | {ON | 1}}

## Query Syntax

    :CALibrate:CALibrator:AOENable?

## Description

This command enables or disables the calibrator output signal to appear on the AUX Out connector.

In the DC level calibrator mode (see `:CALibrate:CALibrator:MODE`), the output signal cannot be enabled on the AUX Out connector. However, this option is available for most AC modes.

## Query Response

    {0 | 1}