# :FUNCtion:PARameters:CTLequalizer:FZP

CTLE Parameters Commands

- :FUNCtion:PARameters:CTLequalizer:ACGain
- :FUNCtion:PARameters:CTLequalizer:BANDwidth
- :FUNCtion:PARameters:CTLequalizer:BWMode
- :FUNCtion:PARameters:CTLequalizer:DBACgain
- :FUNCtion:PARameters:CTLequalizer:DBGain
- :FUNCtion:PARameters:CTLequalizer:DEFinition
- :FUNCtion:PARameters:CTLequalizer:FZP
- :FUNCtion:PARameters:CTLequalizer:GAIN
- :FUNCtion:PARameters:CTLequalizer:GDC
- :FUNCtion:PARameters:CTLequalizer:IMPulse
- :FUNCtion:PARameters:CTLequalizer:POLE
- :FUNCtion:PARameters:CTLequalizer:PRESets
- :FUNCtion:PARameters:CTLequalizer:PRESets:SELections?
- :FUNCtion:PARameters:CTLequalizer:STEP
- :FUNCtion:PARameters:CTLequalizer:TFUNction
- :FUNCtion:PARameters:CTLequalizer:ZERO

## Command Syntax

    :FUNCtionN:PARameters:CTLequalizer:FZP <low-frequency zero-pole>

<low-frequency zero-pole> is a double.

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtionN:PARameters:CTLequalizer:FZP?

## Description

When the Continuous Time Linear Equalizer (CTLE) operator has been selected (`:FUNCtion:FOPerator CTLE`) and the "2 Pole, 2 Gain" CTLE type has been selected (`:FUNCtion:PARameters:CTLequalizer:DEFinition GAIN2`), the `:FUNCtion:PARameters:CTLequalizer:FZP` command specifies the low-frequency zero/pole frequency in Hertz.