# :MEASure:HORizontal:DCYCle:STATus:REASon?

Duty Cycle Commands

- :MEASure:HORizontal:DCYCle
- :MEASure:HORizontal:DCYCle:EDIRection
- :MEASure:HORizontal:DCYCle:FAVorite
- :MEASure:HORizontal:DCYCle:LOCation?
- :MEASure:HORizontal:DCYCle:OCCurrences
- :MEASure:HORizontal:DCYCle:REGion
- :MEASure:HORizontal:DCYCle:SOURce
- :MEASure:HORizontal:DCYCle:STATus?
- :MEASure:HORizontal:DCYCle:STATus:DETails?
- :MEASure:HORizontal:DCYCle:STATus:REASon?
- :MEASure:HORizontal:DCYCle:UREFerence:STATe
- :MEASure:HORizontal:DCYCle:UREFerence:VALue

## Query Syntax

    :MEASure:HORizontal:DCYCle:STATus:REASon?

## Query Response

Refer to the table "Common Reasons for INV or QUES Status".

## Description

Returns a string that explains the reason for a failed `:MEASure:HORizontal:DCYCle` measurement. If the measurement was successful, a null string is returned.

Additional information about the failure may be available using the `:MEASure:HORizontal:DCYCle:STATus:DETails?` sibling query. Use the `:MEASure:HORizontal:DCYCle:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors